Article: Auralization of High-Order Directional Sources from First-Order RIR Measurements (2020)
Authors: Markus Zaunschirm, Franz Zotter, Franck Zagala
Contact: markus.zaunschirm@atmoky.com or zotter@iem.at

Source: Cubelet (array domain), a detailed description and directivity measurements are given in:
(i) 2016_BaumgartnerFaschingGillerKreuzbichler_AkHoloLuGr1.pdf
(ii) https://phaidra.kug.ac.at/o:104374 attn: loudspeaker array is rotated by 45° around x-axis in the measurement.

Receiver: TSL Soundfiled ST450 MK2 (B-format), directivity measurements can be found here: https://phaidra.kug.ac.at/o:68229

Data: LigetiHall_<SOURCE>To<RECEIVER>_Ls<LSIDX>.wav
RIRs to the all channels of the receiving array stored as multichannel 32 Bit wave file with a samplerate of 44.1kHz for one loudspeaker <LSIDX> of the source array.

Setup: see description given in the article

Room: György Ligeti Saal (V=5630 m^3, T60 = 1.4s)
www.kug.ac.at/universitaet/campus-und-gebaeude/mumuth/gyoergy-ligeti-saal-buchungsinformationen/