Article: Auralization of High-Order Directional Sources from First-Order RIR Measurements (2020)
Authors: Markus Zaunschirm, Franz Zotter, Franck Zagala
Contact: markus.zaunschirm@atmoky.com or zotter@iem.at

Source: icosahedral loudspeaker array (IKO), a detailed description and directivity measurements are given in:
(i) http://www.aes.org/e-lib/browse.cfm?elib=19557
(ii) https://ieeexplore.ieee.org/abstract/document/8055161
(iii) https://phaidra.kug.ac.at/o:37785

Receiver: Neumann KU100, directivity measurements can be found here:
https://audiogroup.web.th-koeln.de/FILES/AIA-DAGA2013_HRIRs.pdf
http://audiogroup.web.th-koeln.de/ku100hrir.html

Data: LigetiHall_<SOURCE>To<RECEIVER>_Ls<LSIDX>.wav
RIRs to the all channels of the receiving array stored as multichannel 32 Bit wave file with a samplerate of 44.1kHz for one loudspeaker <LSIDX> of the source array. Here the responses of the left and right channel of the KU100 are stored sequentially for the orientations of (45°,30°,15°,0°,-15°,-30°,-45°).

Setup: see description given in the article

Room: György Ligeti Saal (V=5630 m^3, T60 = 1.4s)
www.kug.ac.at/universitaet/campus-und-gebaeude/mumuth/gyoergy-ligeti-saal-buchungsinformationen/